int yesil\_led=10;

int mavi\_led=9;

int kirmizi\_led=8;

void setup()

{

pinMode(yesil\_led, OUTPUT);

pinMode(mavi\_led, OUTPUT);

pinMode(kirmizi\_led, OUTPUT);

}

void loop()

{

digitalWrite(kirmizi\_led, HIGH);

digitalWrite(mavi\_led, LOW);

digitalWrite(yesil\_led, LOW);

delay(1000);

digitalWrite(kirmizi\_led, LOW);

digitalWrite(mavi\_led, HIGH);

digitalWrite(yesil\_led, LOW);

delay(1000);

digitalWrite(kirmizi\_led, LOW);

digitalWrite(mavi\_led, LOW);

digitalWrite(yesil\_led, HIGH);

delay(1000);

digitalWrite(kirmizi\_led, HIGH);

digitalWrite(mavi\_led, HIGH);

digitalWrite(yesil\_led, LOW);

delay(1000);

digitalWrite(kirmizi\_led,LOW);

digitalWrite(mavi\_led, HIGH);

digitalWrite(yesil\_led, HIGH);

delay(1000);

digitalWrite(kirmizi\_led, HIGH);

digitalWrite(mavi\_led, LOW);

digitalWrite(yesil\_led, HIGH);

delay(1000);

digitalWrite(kirmizi\_led, HIGH);

digitalWrite(mavi\_led,HIGH);

digitalWrite(yesil\_led, HIGH);

delay(1000);

digitalWrite(kirmizi\_led, LOW);

digitalWrite(mavi\_led, LOW);

digitalWrite(yesil\_led, LOW);

delay(1000);

}